**ECE 385**

**2021 FA**

**LAB 9**

**SOC with Advanced Encryption Standard in SystemVerilog**

Zhou Qishen, Xie Mu

**Introduction**

The **AES** (**Advanced Encryption Standard**) is the most common symmetric encryption algorithm. In the Lab 9, we realize an AES-128 encryption/decryption on the NIOS 2 soc with FPGA board. The encryption part is done in software while the description part is done in the hardware. We also write benchmarks of the whole progress, and we can find that the hardware description is much faster than the software encryption.

**Description & Diagram**

**Summarize the operation of the AES encryption and decryption**

The AES is a symmetry encryption algorithm, as a result, both the sender and the receiver should know the Cipher key. In order to use the AES, you should prepare a Cipher key and the Plaintext, that is the message to be encrypted, and load it to the AES encryption, and then we get the encrypted message called Ciphertext. The receiver who has the Cipher key and the Cyphertext can goes through the reverse algorithm to produce the original meaningful Plaintext message.

**Description and the operation of the AES encryptor/decryptor.**

* 1. Software encryption

The message is encrypted by a C program running on the NIOS 2. With the JTAG UART module, we can get a scanf function, so we can interact to it with the console to send Plaintext and the Cipher key that we prefer. Once you send a valid message and a key, the main function will call the function CharToHex to convert the strings to the hex values, Then the key expansion function will expand the key to 10 round keys, and then we add the first Round Key with XOR to the message. Then we will loop the following steps for 9 times to encrypt the message totally: execute the SubBytes, ShiftRows, MixColumns and then addRoundKey. The SubBytes function will substitute the value based on the look up table with High four bits and the low 4 bits of the original value. The ShiftRows function will left shift the values in each row based on the number of the row. The MixColumns function will multiply each column with a fix matrix in the GF(2^8) to get the fixed value. After the loop, we call SubBytes, ShiftRows, and addRoundKey again to output the final Ciphertext.

* 1. Hardware description

The Ciphertext will be decrypted by hardware logics written by System Verilog on the FPGA. When we type in the CipherKey and the Ciphertext in the console, the software will write them to the register file that defined in the AES decryption module. Then we initiate the AES module and all the linked module and then define states to decryption step by step. According to the diagram, we should start with the key expansion module to expand 9 round keys. Then we run addRoundKey module to do XOR to the keys. After that we will loop the invSubBytes, InvShiftRows, AddRoundKeys, and InvMixColumns 9 times to completely reverse the encryption. Then We will do InvShiftRows, InvSubBytes and AddRoundKeys again to get the Plaintext again.

* 1. Description of the hardware/software interface

We connect the hardware and software with the module Avalon\_aes\_interface.sv. We create a 32-bit reg file with 16 slot to hold the intermediates. After the software finish the encryption. The key will be stored in the first 4 registers and the encrypted message will be stored in the next 4 registers. After the hardware finish the description, the decrypted message will be store in the next 4 registered. Then we will use the 12 and 13 slot to hold signals that sent through registers, and register 14 will be used to hold START signal that given by the C program. To control the registers, the NIOS 2 will write pointers to sent messages to the target slot.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

**System Level Block Diagram**

A picture containing diagram

Description automatically generated

Block Diagram

**State Diagram of AES decrypted controller**

Diagram

Description automatically generated

State Diagram

**Hardware Module Description**

**Module: sdram**

Input: clk, reset, s1

Output: wire

Description: This module is a 32-bit dynamic memory of SOC, which contains 1 chip, 4 banks, 13 rows and 10 columns, with the size of 1GB data.

Purpose: It is used for store data and address.

**Module: onchip\_memory2\_0**

Input: clk, reset, s1, wire

Output: readdata

Description: This module is writable RAM with memory size of 16 byte and datawidth of 32.

Purpose: This module is the on chip memory of NOIS II processor.

**Module: led**

Input: clk, reset, s1

Output: external\_connection

Description: The module of LED on DE2 board with 8-bit datawidth.

Purpose: This module is used for control the LED on board to output data.

**Module: sdram\_pll**

Input: inclk\_interface, inclk\_interface\_reset, pll\_slave, c0

Output: c1

Description: Clock module with the offset of -3 ns.

Purpose: This module is used for adjusting the clock input and I/O of sdram.

**Module: sysid\_qsys\_0**

Input: clk, reset, control\_slave

Output: almost\_empty, almost\_full, empty, full, rd\_data

Description: This module is system ID checker to ensure the compatibility between hardware and software.

Purpose: It can prevents us from loading software onto an FPGA which

has an incompatible NIOS II configuration.

**Module: nios2\_gen2\_0**

Input: clk, reset, data\_master, instruction\_master, irq, debug\_deset\_request, debug\_mem\_slave

Output: custrom\_instruction\_master

Description: The build-in NIOS II/e processor.

Purpose: The main processor of the SOC system.

**Module: jtag\_uart\_0**

Input: clk, reset, avalon\_jtag\_slave

Output: irq

Description: It is a build-in JTAG UART peripheral module.

Purpose: This module enable use the terminal of the host computer to communicate with the NIOS II

**Module: timer**

Input: clk, reset, s1

Output: irq

Description: Nois II built-in timer that can track the program operation time.

Purpose: This module is used to record the hardware decrypting time.

**Module: AES**

Input: CLK, RESET, AES\_START, AES\_KEY AES\_MSG\_ENC,

Output: AES\_DONE, AES\_MSG\_DEC

Description: AES algorism that be implemented in hardware.

Purpose: This module is used to carry out the main job in hardware decrypting message.

**Module: AddRoundKey**

Input: state, roundKey

Output: out

Description: It is one of submodule of AES.

Purpose: This module is used to apply a Round Key of 4-Word matrix to the updating State through a simple XOR operation in every round.

**Module: avalon\_aes\_interface**

Input: CLK, RESET, AVL\_READ, AVL\_WRITE, AVL\_CS, AVL\_BYTE\_EN, AVL\_WRITEDATA

Output: AVL\_READDATA, EXPORT\_DATA

Description: This is the interface between Avalon and AES module.

Purpose: This module enable the communication between NOIS II and AES module.

**Module: hexdriver**

Input: In

Output: Out

Description: It is used for storing the value in hex display.

Purpose: This module is used to display the highest digest and lowest digits in message.

**Module: InvMixColumns**

Input: in

Output: out

Description: It is one of submodule of AES.

Purpose: This module is used to perform the inverse operation of MixColumns.

**Module: InvShiftRows**

Input: data\_in

Output: data\_out

Description: It is one of submodule of AES.

Purpose: This module is designed for carrying out the inverse operation of ShiftRows in encrypting.

**Module: KeyExpansion**

Input: clk, Cipherkey

Output: KeySchedule

Description: It is one of submodule of AES.

Purpose: This module is used to takes the Cipher Key and performs a Key Expansion to generate a series of Round Keys and store them into Key Schedule.

**Module: SubBytes**

Input: clk, in

Output: out

Description: It is one of submodule of AES.

Purpose: Each Byte of the updating State is non-linearly transformed by taking the

multiplicative inverse in Rijndael’s finite field then applying an affine transformation. This module provides a look-up table for the transformation.

**Simulation**

A picture containing timeline

Description automatically generated

**Post-Lab**

**Document the Design Resources and Statistics in following table.**

|  |  |
| --- | --- |
| Property | Value |
| LUT | 7175 |
| DSP | 0 |
| Memory | 125952 |
| Flip-Flop | 2806 |
| Static Power | 102.53 mW |
| Dynamic Power | 72.09 mW |
| Total Power | 242.72 mW |

**Answer to two hidden questions**

**Q: Which would you expect to be faster to complete encryption/decryption, the**

**software or hardware? Is this what your results show?**

We think that the hardware will operate a faster speed, since the algorism is implemented much directly, without much delay at interfaces or ports.



And our test result backs up our idea that hardware encryption is much more efficient.

**Q: If you wanted to speed up the hardware, what would you do? (Not**

We can speed up by modifying the InvMixMatrix part. In the lab, we use 4 states to calculate the inverse mix matrix column by column. As a result, if we can reduce the calculation state, we can save much clock edge to decrypt the message.

**Conclusion**

The project works correctly on both the weeks, but it was hard to design the decryption states for hardware decryption since there are a lot of modules to design. This lab help me understand the hardware can process data much faster than the software when the date procession can be design in logics. I think we can do some different encryption next time like RSA.